REQUEST FOR PROPOSAL (RFP)
Labor and Materials – Bid Category 32-01 Site Concrete
Van Buren Public Schools – Operations Building / Bus Garage
Issued By: Davenport Brothers Construction Co., Inc.
Construction Manager: Granger Construction Company
Owner: Van Buren Public Schools
Project: Operations Building / Bus Garage
Project Location: 13770 Haggerty Road, Van Buren Township, Michigan 48111
Bid Category: 32-01 Site Concrete (Labor Only)
Proposal Type: Lump Sum Labor Proposal

INVITATION TO BID
Davenport Brothers Construction Co., Inc., acting as General Contractor to bid to Granger Construction Company, is soliciting proposals from qualified concrete contractors to provide all labor, supervision, tools, equipment, and incidental materials required for the complete installation of the Site Concrete scope for the Van Buren Public Schools Operations Building / Bus Garage Project.
This is a Labor-Only Bid Package. Major concrete materials may be supplied by others or procured separately at Davenport Brothers Construction's discretion. The subcontractor shall include all labor, equipment, layout, forming, placement, finishing, curing, and coordination necessary for a complete installation. [32-01 SITE CONCRETE | PDF], [VBPS Opera...07-15-2026 | PDF]

SCOPE OF WORK
The successful subcontractor shall provide all labor, supervision, equipment, tools, layout, and field engineering required for complete installation of all Site Concrete work including but not limited to:
Concrete Paving
· Reinforced concrete pavement.
· Standard concrete pavement.
· Sidewalks.
· Concrete aprons.
· Curb and gutter systems.
· Building perimeter concrete mow strip.
· Frost-free stoops and foundations.
· Concrete equipment pads.
· Concrete housekeeping pads.
· Concrete apron around light poles.
· Detectable warning surfaces at ADA locations. [32-01 SITE CONCRETE | PDF]

Concrete Installation Responsibilities
Provide labor and equipment for:
· Layout and surveying.
· Forming.
· Reinforcing placement.
· Wire mesh installation.
· Chairs and supports.
· Concrete placement.
· Finishing.
· Joint installation.
· Saw cutting.
· Expansion joints.
· Control joints.
· Curing and protection.
· Backer rod installation.
· Joint sealant installation.
· Epoxy doweling.
· Drilling and anchoring.
· Cleanup and punch list completion. [32-01 SITE CONCRETE | PDF]

Site Equipment Pads
Provide labor for installation of:
· Generator pad.
· DTE transformer pad.
· ACCU-1 pad.
· HP-1 pad.
· HP-2 pad.
· Exterior concrete housekeeping pads.
Include separate mobilizations as necessary to accommodate equipment delivery schedules. [32-01 SITE CONCRETE | PDF]

Snow Melt Area
Coordinate with Mechanical Contractor for installation of snow melt tubing systems.
Concrete subcontractor shall provide labor associated with:
· Placement around tubing.
· Reinforcement installation.
· Insulation placement.
· Finishing and protection of installed system. [32-01 SITE CONCRETE | PDF]

Bollards
Install all exterior bollards furnished by others.
Coordinate installation with:
· Underground utilities.
· Downspouts.
· Snow melt tubing.
· Concrete foundations. [32-01 SITE CONCRETE | PDF]

Monument Sign & Flagpole Lighting Foundations
Provide labor for:
· Excavation.
· Formwork.
· Reinforcing placement.
· Concrete placement.
For foundations serving:
· Monument sign flood lights.
· Flag pole flood lights. [32-01 SITE CONCRETE | PDF]

MATERIALS SUPPLIED BY OTHERS
Unless specifically noted otherwise, the following may be owner or GC supplied:
· Ready-mix concrete.
· Reinforcing steel.
· Wire mesh.
· Expansion material.
· Joint sealants.
· Detectable warning panels.
· Bollards.
Subcontractor shall include unloading, handling, installation, and protection of supplied materials. [32-01 SITE CONCRETE | PDF]

SPECIFICATIONS INCLUDED
This RFP includes the requirements of:
· Division 00
· Division 01
· 03 1000 Concrete Forming and Accessories
· 03 2000 Concrete Reinforcing
· 03 3000 Cast-In-Place Concrete
· 07 2100 Thermal Insulation
· 07 9200 Joint Sealants
· 32 1313 Concrete Paving
· 32 1373 Concrete Paving Joint Sealants
· 32 1726 Detectable Warning Surfaces
· Applicable civil, structural, architectural and MEP drawings. [32-01 SITE CONCRETE | PDF], [VBPS Opera...07-15-2026 | PDF]

EXCLUSIONS
The following are excluded from this subcontract:
· Monument sign footing by Structural Concrete Contractor.
· Furnishing of exterior bollards.
· Light pole bases.
· Asphalt paving.
· Pavement striping.
· Site furnishings.
· Flagpole foundation by others.
· Underground utility work by Earthwork Contractor. [32-01 SITE CONCRETE | PDF]

SAFETY REQUIREMENTS
Subcontractor shall comply with:
· OSHA requirements.
· MIOSHA requirements.
· Granger Construction Safety Program.
· Davenport Brothers Construction Safety Policies.
· Fall Protection Standards.
· Silica Exposure Control Requirements. [32-01 SITE CONCRETE | PDF], [VBPS Opera...07-15-2026 | PDF]
Requirements include:
· Competent person on site at all times.
· Daily jobsite inspections.
· Weekly toolbox talks.
· Concrete washout compliance.
· Dust control measures.
· Proper PPE utilization.

SCHEDULE REQUIREMENTS
Subcontractor shall provide:
· Mobilization date.
· Crew size.
· Production schedule.
· Pour sequence.
· Equipment list.
· Recovery plan if behind schedule.
Failure to maintain schedule may require:
· Additional manpower.
· Extended work hours.
· Weekend work.
· Multiple crews at no additional cost if required to recover schedule impacts caused by subcontractor delays.

PREVAILING WAGE REQUIREMENTS
This project is subject to Michigan Prevailing Wage requirements.
Subcontractor shall:
· Pay prevailing wages.
· Submit certified payroll reports.
· Maintain labor classifications.
· Comply with all wage reporting requirements. [32-01 SITE CONCRETE | PDF], [VBPS Opera...07-15-2026 | PDF]

INSURANCE REQUIREMENTS
Provide current certificates showing:
· General Liability: $2,000,000 Minimum
· Automobile Liability: $1,000,000
· Workers Compensation: Statutory
· Umbrella Liability: $5,000,000 Minimum
Davenport Brothers Construction Co., Inc., Granger Construction Company, and Van Buren Public Schools shall be named as Additional Insureds.

WARRANTY
Provide:
· Two (2) Year Labor Warranty
Warranty period shall commence upon Project Substantial Completion. [32-01 SITE CONCRETE | PDF]

REQUIRED ALTERNATE PRICING
Provide separate pricing for:
Alternate G-2
· Expansion paper.
· Backer rod.
· Joint sealants around Bus Canopy foundations.
· Concrete foundations and bollard infill for EV charging stations. [32-01 SITE CONCRETE | PDF]
Alternate G-4
· Manual Transfer Switch (MTS-2) housekeeping pad.
· Concrete foundations.
· Bollard infill.
· Associated joint sealants. [32-01 SITE CONCRETE | PDF]

UNIT PRICING
Provide labor unit pricing for:
· Additional 5" Concrete Sidewalk ($/SF)
· Additional Curb & Gutter ($/LF) [32-01 SITE CONCRETE | PDF]

PROPOSAL SUBMITTAL REQUIREMENTS
Submit proposal including:
1. Lump Sum Labor Price.
2. Crew Size.
3. Superintendent Resume.
4. EMR Rating.
5. Insurance Certificate.
6. Three Similar Project References.
7. Equipment List.
8. Schedule Duration.
9. Acknowledgment of Drawings/Addenda.
10. Alternate Pricing.
11. Unit Pricing.
Proposal Subject: VBPS Operations Building / Bus Garage – 32-01 Site Concrete Labor Only Proposal
Attention: Mark Davenport
Davenport Brothers Construction Co., Inc.
END OF RFP

