REQUEST FOR PROPOSAL (RFP)
Labor Only – Bid Category 13-01 Pre-Engineered Metal Building (PEMB)
Van Buren Public Schools – Operations Building / Bus Garage
Construction Manager: Granger Construction Company
Issued By: Davenport Brothers Construction Co., Inc.
Project: Van Buren Public Schools – Operations Building / Bus Garage
Owner: Van Buren Public Schools
Construction Manager: Granger Construction Company
Project Location: 13770 Haggerty Road, Van Buren Township, MI 48111
Bid Package: 13-01 Pre-Engineered Metal Building – Labor Only
Date: July 2026

1. Invitation to Bid
Davenport Brothers Construction Co., Inc., acting as General Contractor to bid to Granger Construction Company, is soliciting sealed proposals from qualified union or non-union steel erection contractors for the labor-only erection and installation of the Pre-Engineered Metal Building (PEMB) for the Van Buren Public Schools Operations Building / Bus Garage project.
Subcontractors shall provide all labor, supervision, tools, equipment, cranes, rigging, safety equipment, temporary protection, and incidental materials required to completely erect the PEMB system furnished by others in accordance with the Contract Documents.

2. Scope of Work
The successful subcontractor shall furnish all labor and services necessary for complete erection of the PEMB system, including but not limited to:
Structural Framing
· Erection of PEMB primary frames.
· Installation of columns, rafters, girts, purlins, bracing, and secondary framing.
· Installation of mezzanine support beams provided within PEMB scope.
· Alignment, plumbing, bolting, and final tightening of all framing.
Roof System
· Installation of standing seam roofing system.
· Installation of roof insulation systems.
· Installation of roof trim, closure strips, ridge assemblies, and accessories.
· Temporary roof fall protection compliant with MIOSHA and Granger Safety Program.
Wall System
· Installation of exterior metal wall panels.
· Installation of insulated wall assemblies.
· Installation of corner trim, base trim, rake trim, jamb trim, and associated flashings.
Building Enclosure
· Installation of gutters and downspouts.
· Weatherproofing of PEMB envelope.
· Installation of sealants and closure materials required by manufacturer.
· Water-tight completion of building envelope.
Coordination Requirements
· Coordinate all openings required for: 
· Doors
· Overhead doors
· Louvers
· Windows
· Mechanical penetrations
· Electrical penetrations
· Plumbing penetrations
· Exhaust fans
· Roof curbs
Miscellaneous
· Install steel framing at entrance canopies as required.
· Coordinate flashing of MEP penetrations.
· Install fire stopping associated with PEMB penetrations.
· Participate in BIM coordination meetings.
· Perform punch list corrections and final adjustments.

3. Materials Furnished by Others
The following items will be furnished and delivered to the project site by others:
· Pre-Engineered Metal Building package.
· Structural steel components included in PEMB package.
· Roof panels.
· Wall panels.
· Trim and flashing materials.
· Fasteners and erection hardware supplied by PEMB manufacturer.
· Anchor bolts previously installed by the concrete contractor.
Subcontractor shall:
· Receive materials.
· Verify shipments.
· Protect materials.
· Report shortages immediately.
· Assume responsibility for material damage occurring after acceptance.

4. Exclusions
The following are excluded from this labor-only subcontract:
· Material purchase of PEMB package.
· Underground downspout connections.
· Roofing membrane at man door canopies.
· Mezzanine steel specified under Bid Package 05-01 Miscellaneous Steel.
· Structural concrete work.
· Crane pads and haul roads provided by Earthwork Contractor.

5. Safety Requirements
Subcontractor shall comply with:
· MIOSHA requirements.
· OSHA regulations.
· Granger Construction Safety & Health Program.
· Davenport Brothers Construction Safety Policies.
· Fall Protection Standards.
· Site-specific safety orientation requirements.
Requirements include:
· 100% tie-off.
· Competent person onsite at all times.
· Daily safety inspections.
· Weekly toolbox talks.
· Job Hazard Analysis (JHA).
· Safety Data Sheets (SDS).

6. Prevailing Wage Requirements
This project is subject to Michigan Prevailing Wage requirements.
Subcontractor shall:
· Pay all required prevailing wages and fringes.
· Submit certified payroll reports.
· Maintain labor classifications.
· Provide wage compliance documentation upon request.

7. Schedule Requirements
Subcontractor shall provide:
· Detailed manpower loading schedule.
· Mobilization date.
· Erection duration.
· Roofing duration.
· Dry-in milestone date.
· Substantial completion date.
Subcontractor shall confirm ability to meet all Granger milestone dates.

8. Proposal Requirements
Provide a Lump Sum Labor Proposal Including:
Labor
· Field labor.
· Supervision.
· Foremen.
· Safety personnel.
Equipment
· Cranes.
· Telehandlers.
· Aerial lifts.
· Safety systems.
· Rigging equipment.
Administration
· BIM participation.
· Daily reports.
· Coordination meetings.
· Procore utilization.
Include Separate Pricing For:
· Alternate G-2 Bus Canopy PEMB Erection.
· Overtime rates.
· Weekend rates.
· Additional manpower rates.

9. Required With Proposal
Submit:
1. Company Profile.
2. EMR for last three years.
3. MIOSHA recordable rate.
4. Current insurance certificates.
5. Bonding capacity letter.
6. Three comparable PEMB projects completed within the last five years.
7. Proposed project superintendent resume.
8. Manpower loading plan.
9. Equipment list.
10. Acknowledgment of all project addenda.

10. Insurance Requirements
Subcontractor shall maintain:
· Commercial General Liability: $2,000,000 Minimum.
· Automobile Liability: $1,000,000.
· Workers Compensation: Statutory.
· Umbrella Liability: $5,000,000 Minimum.
Davenport Brothers Construction Co., Inc., Granger Construction Company, and Van Buren Public Schools shall be named as Additional Insureds.

11. Warranty
Provide a minimum:
· Two (2) Year Labor Warranty.
Warranty period shall commence at Project Substantial Completion.

12. Proposal Delivery
Submit proposal to:
Davenport Brothers Construction Co., Inc.
Attn: Mark Davenport
Estimator / Project Executive
Proposal shall clearly reference:
"VBPS Operations Building / Bus Garage – Bid Category 13-01 PEMB Labor Only"

Scope Basis
This RFP is based upon:
· Granger Construction Bid Category 13-01 Pre-Engineered Metal Building.
· Division 00 and Division 01 requirements.
· Specification Section 13 3419 Pre-Engineered Metal Building Systems.
· Drawings and specifications dated June 26, 2026.
· Granger Bid Package issued July 15, 2026.

